1. Open python ‘quad\_server’ and run it in background. See that the message appears in localhost:5000 in browser
2. Run ‘ngrok http 5000’ in the ngrok folder to generate the port exposure
3. Input the new web address into twilio
4. See that the localhost:5000 matches the ngrok page and see in terminal a response’
5. Text!
6. Should get feedback from the resp.Response() type
7. Should see last command in the ‘commands.txt’ file for matlab to find

Needed libraries

Flask

Twilio.twiml

Ngrok

All located in the project folder. Make sure matlab address to the command.txt is updated